****

**DATA CERTIFICATE**

**for trailer O1/O2 (goods), trailer for motorcycle or moped,**

**towed equipment or caravan, all with a max mass of 3.500 kg**

Make:       Type designation:       Model:       Variant:

Vehicle Identification No.:       Date of first registration\*:       or new [ ]

[ ]  Trailer O1 (goods) [ ]  Trailer O2 (goods) [ ]  Towed equipment

[ ]  Caravan [ ]  Trailer for a mc [ ]  Trailer for a moped

Mass (dry):      kg (if 1. reg. after 04.12.05 only needed for caravan)

Actual mass (EU):      kg

Technically permissible laden mass:      kg

Technically permissible mass, axle/axle group:      kg

Technically permissible mass at the coupling point:     kg

The trailer is constructed to a speed of:     km/h

[ ]  The trailer has no brakes

[ ]  The trailer has brakes, where the inertia control device, the transmission to the brakes and wheel brakes fulfils the rules in ECE Regulation 13 and gives a braking rate of not less than 50%

The trailer must have a rigid drawbar\*\*

**The informations are confirmed:**

(Vehicle manufacturer, the manufacturers representative, a technical service or an approved testing laboratory)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|       |  |  |  |  |
| \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| (date) |  | (company/stamp incl. adress) |  | (name and signature) |

All data must apply to the vehicle, as it was, when it left the basic manufacturer. Every fields must be filled out.

Data-relevant technical modifications requires separate additional documentation for fulfilling the rules in the Danish Detailed Regulations for Vehicles according to the finally approved date of 1. registration.

\* Year of manufacture, if the time of first registration is not known. The vehicle shall be considered as registrated first time the 1. of January that year

This Data Certificate may be utilised for new and used trailers.

\*\* A trailer with hinged drawbar (full trailer) and inertia brakes cannot be approved due to stability matters